FURNITURE IN-HOUSE TEST REPORT
Top Systems Group Inc. | Quality Assurance Department
	1. PRODUCT & TEST IDENTIFICATION



	Factory / Supplier
	____________________________
	Agent
	____________________________

	Customer
	____________________________
	Product Description
	____________________________

	Item Number
	____________________________
	Version / Revision
	____________________________

	Test Date
	____________________________
	Tester(s)
	____________________________

	Product Dimensions
	________ x ________ x ________
	Net Weight
	________ kg

	Product Photo
	Insert product photo
	Overall Test Result
	PASS / FAIL / PENDING


	2. PRODUCT SPECIFICATION / TEST PROTOCOL



	Product Specification
	Record the product details relevant to the test, including material / construction / component thickness / other applicable requirements.

	Test Protocol Used
	1. ______________________________
2. ______________________________
3. ______________________________

	Testing Scope
	Record the tests performed and identify any test marked Not Applicable with the reason.




	3. TEST SUMMARY



	#
	Test
	Status
	Remarks

	1
	Interlock Systems Test
	PASS / FAIL / N.A.
	

	2
	Stability - Simulated Clothing Load
	PASS / FAIL / N.A.
	

	3
	Stability - Horizontal Dynamic Force
	PASS / FAIL / N.A.
	

	4
	Stability - Carpet / Child Weight
	PASS / FAIL / N.A.
	

	5
	Recommended Load Test
	PASS / FAIL / N.A.
	

	6
	Storage Unit Drop Test
	PASS / FAIL / N.A.
	

	7
	Distributed Functional Load
	PASS / FAIL / N.A.
	

	8
	Distributed Proof Load
	PASS / FAIL / N.A.
	

	9
	Extendible Element Functional Load
	PASS / FAIL / N.A.
	

	10
	Extendible Element Proof Load
	PASS / FAIL / N.A.
	


	4. TEST SETUP / APPLICABILITY RECORD



	Field
	Entry / Requirement
	Field
	Entry / Requirement

	Applicable Standard(s)
	____________________________
	Customer / Project Protocol
	____________________________

	Test Sample Condition
	New / Production Sample / Other
	Test Location
	____________________________

	Test Equipment
	____________________________
	Calibration / Verification
	____________________________

	Pre-Test Condition
	Record assembly / configuration before testing.
	Post-Test Condition
	Record condition after testing.




	1. TEST TO EVALUATE INTERLOCK SYSTEMS



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	1. Test to Evaluate Interlock Systems
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Apply 30 lb horizontal pull force on each interlocked extendible element. Force shall be applied over a period of at least 5 s and held for 10 s.

	Test Method / Setup
	Record point of application, force, fixture / setup and measured dimensions as applicable.

	Calculation / Applied Load
	Enter applied force / measured result / calculation if applicable.

	Test Duration
	At least 5 s application and 10 s hold.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 1 - Photo 1

INSERT PHOTO



	Test 1 - Photo 2

INSERT PHOTO




	Test 1 - Photo 3

INSERT PHOTO



	Test 1 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	2. STABILITY TEST - SIMULATED CLOTHING LOAD



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	2. Stability Test - Simulated Clothing Load
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Use the applicable non-extendible / extendible element loading requirement. Record the density / loading basis and the applied test weight.

	Test Method / Setup
	Load the applicable drawer / storage element(s), record dimensions used in the calculation, and test for the required period.

	Calculation / Applied Load
	Example source format: density x element volume = calculated load; record actual test weight separately.

	Test Duration
	30 s, or applicable project requirement.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 2 - Photo 1

INSERT PHOTO



	Test 2 - Photo 2

INSERT PHOTO




	Test 2 - Photo 3

INSERT PHOTO



	Test 2 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	3. STABILITY TEST - SIMULATED HORIZONTAL DYNAMIC FORCE



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	3. Stability Test - Simulated Horizontal Dynamic Force
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Apply the specified horizontal pull force at the applicable reach point / height. Source example uses 10 lb force at a height less than 56 in (1422 mm).

	Test Method / Setup
	Record highest reach point on the applicable front / handle and actual force applied.

	Calculation / Applied Load
	Record measured reach point and actual force / load.

	Test Duration
	At least 5 s application and 10 s hold.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 3 - Photo 1

INSERT PHOTO



	Test 3 - Photo 2

INSERT PHOTO




	Test 3 - Photo 3

INSERT PHOTO



	Test 3 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	4. STABILITY TEST - SIMULATING A REACTION ON CARPET WITH CHILD WEIGHT



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	4. Stability Test - Simulating a Reaction on Carpet with Child Weight
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Hang the required test weight on the extended top drawer / door, one drawer or door at a time while the rest are open, where applicable. Record block placement.

	Test Method / Setup
	Record specified test weight and actual load, block dimensions / height and placement position.

	Calculation / Applied Load
	Record required weight versus actual test load and support / block dimensions.

	Test Duration
	Per applicable protocol.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 4 - Photo 1

INSERT PHOTO



	Test 4 - Photo 2

INSERT PHOTO




	Test 4 - Photo 3

INSERT PHOTO



	Test 4 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	5. CUSTOMER / PROJECT RECOMMENDED LOAD TEST



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	5. Customer / Project Recommended Load Test
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record the customer / project recommended load. The source example used a 24-hour recommended load test.

	Test Method / Setup
	Apply the required load to the specified top / drawer / storage area and record actual test weight.

	Calculation / Applied Load
	Record target load, calculated basis if applicable, and actual load.

	Test Duration
	Enter required duration; source example: 24 hours.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 5 - Photo 1

INSERT PHOTO



	Test 5 - Photo 2

INSERT PHOTO




	Test 5 - Photo 3

INSERT PHOTO



	Test 5 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	6. STORAGE UNIT DROP TEST



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	6. Storage Unit Drop Test
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record drop height and product weight. The source example used a 7.1 inch drop height.

	Test Method / Setup
	Measure / verify drop height, product weight and test setup. Photograph pre-test and post-test condition.

	Calculation / Applied Load
	Record nominal drop height and measured height; record product NW.

	Test Duration
	Enter required drop sequence / number of drops.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 6 - Photo 1

INSERT PHOTO



	Test 6 - Photo 2

INSERT PHOTO




	Test 6 - Photo 3

INSERT PHOTO



	Test 6 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	7. DISTRIBUTED FUNCTIONAL LOAD



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	7. Distributed Functional Load
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record the applicable functional load basis for top, storage and extendible elements. Source example: Top 141 kg/m2; Storage 470 kg/m3; Extendible Element 470 kg/m3.

	Test Method / Setup
	Calculate the load from the applicable surface area / volume, then record actual test weight.

	Calculation / Applied Load
	Show calculation and actual load. Example: density x dimensions = required load.

	Test Duration
	Source example: 60 minutes.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 7 - Photo 1

INSERT PHOTO



	Test 7 - Photo 2

INSERT PHOTO




	Test 7 - Photo 3

INSERT PHOTO



	Test 7 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	8. DISTRIBUTED PROOF LOAD



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	8. Distributed Proof Load
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record the applicable proof load basis. Source example: Top 211 kg/m2; Storage 720 kg/m3; Extendible Element 470 kg/m3.

	Test Method / Setup
	Apply the required proof load and monitor product condition / serviceability.

	Calculation / Applied Load
	Show calculation and actual proof load.

	Test Duration
	Source example: 15 minutes.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 8 - Photo 1

INSERT PHOTO



	Test 8 - Photo 2

INSERT PHOTO




	Test 8 - Photo 3

INSERT PHOTO



	Test 8 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	9. EXTENDIBLE ELEMENT FUNCTIONAL LOAD TEST



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	9. Extendible Element Functional Load Test
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record the applicable extendible element functional load basis. Source example: 470 kg/m3.

	Test Method / Setup
	Apply calculated load to the drawer / extendible element; test open and closed positions.

	Calculation / Applied Load
	Show calculation, actual test weight and condition after test.

	Test Duration
	Source example: 60 minutes open, 60 minutes closed.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 9 - Photo 1

INSERT PHOTO



	Test 9 - Photo 2

INSERT PHOTO




	Test 9 - Photo 3

INSERT PHOTO



	Test 9 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	10. EXTENDIBLE ELEMENT PROOF LOAD TEST



	Test No. / Test Name
	Applicability
	Result
	Reference / Protocol

	10. Extendible Element Proof Load Test
	Applicable / N.A.
	PASS / FAIL / PENDING
	Enter applicable standard / customer / project protocol


	Test Requirement
	Record the applicable extendible element proof load basis. Source example: 720 kg/m3.

	Test Method / Setup
	Apply calculated proof load to the drawer / extendible element; test open and closed positions.

	Calculation / Applied Load
	Show calculation, actual test weight and condition after test.

	Test Duration
	Source example: 15 minutes open, 15 minutes closed.



	Required / Target
	Actual / Measured
	Condition After Test
	Serviceability
	Result

	
	
	No visible damage / record condition
	No loss of serviceability / record finding
	PASS / FAIL / PENDING



	Test 10 - Photo 1

INSERT PHOTO



	Test 10 - Photo 2

INSERT PHOTO




	Test 10 - Photo 3

INSERT PHOTO



	Test 10 - Photo 4

INSERT PHOTO





Photo evidence / observations
Test Observation / Conclusion: ____________________________________________________________________________________________
____________________________________________________________________________________________


	11. FINAL TEST CONCLUSION



	Overall Test Result
	PASS / FAIL / PENDING
	Loss of Serviceability
	YES / NO

	Structural / Functional Damage
	YES / NO
	Retest Required
	YES / NO

	Open Corrective Action
	____________________________
	Target Date
	____________________________

	Tester(s)
	____________________________
	Test Date
	____________________________

	Prepared by
	____________________________
	Date
	____________________________


	12. TEST EQUIPMENT / MEASUREMENT RECORD



	Equipment
	Identification / Model
	Calibration / Verification
	Remarks

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


	13. FINAL REMARKS



________________________________________________________________________________________________
________________________________________________________________________________________________
________________________________________________________________________________________________
________________________________________________________________________________________________
________________________________________________________________________________________________
Top Systems Group Inc. | Quality Assurance Department | Prepared by: __________ | Date: __________ | Page  of 




